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Notes to Specifier:

1. Where several alternative parameters or specifications exist, or where, the specifier has the option of selecting and inserting text, such choices are presented in <bold text>.

2. Explanatory notes and comments are presented in italic text.

3. If there are any changes between the previous version of this document & this updated version (2020), they are listed on the last page of this document.


















NETWORKING SWITCHES

[bookmark: PART__1_GENERAL]PART 1	GENERAL
1.01 Summary
A	This specification describes a 1U rack-mount enterprise class Networking Switch.
1.02 Related Requirements
A	23 00 00 Heating, Ventilating, and Air Conditioning (HVAC)
1. 23 70 00	Central HVAC Equipment
2. 23 80 00	Decentralized HVAC Equipment B	27 00 00	Communications
1. 27 05 00	Common Work Results for Communications
2. 27 11 16	Communications Cabinets, Racks, Frames, and Enclosures
3. 27 15 01	Communications Horizontal Cabling Applications
a. 27 15 01.13	Video Surveillance Communications Conductors and Cables
4. 27 21 00	Data Communications Network Equipment
C	28 01 00	Operation and Maintenance of Electronic Safety and Security
1. 28 01 20	Operation and Maintenance of Video Surveillance D	28 05 00	Common Work Results for Electronic Safety and Security
	1. 28 05 07
	Power Sources for Electronic Safety and Security

	2. 28 05 09
	Surge Protection for Electronic Safety and Security

	3. 28 05 11
	Cyber Security Requirements for Electronic Safety and Security

	4. 28 05 17
	Workstations for Electronic Safety and Security

	5. 28 05 19
	Storage Appliances for Electronic Safety and Security

	6. 28 05 31
	Communications Equipment for Electronic Safety and Security

	7. 28 05 45
	Systems Integration and Unified Systems


E 28 06 00	Schedules for Electronic Safety and Security
F 28 08 00	Commissioning of Electronic Safety and Security G	28 20 00	Video Surveillance
1.03 References
A	Abbreviations
1. Gb/s - Gigabit per second
2. GigE - Gigabit Ethernet
3. GB – Gigabyte
4. GPU – Graphics Processing Unit
5. HDD - Hard Disk Drive
6. iDRAC - Integrated Dell Remote Access Controller
7. LAN - Local Area Network
8. LOM – LAN on Motherboard
9. LRDIMM - Load-Reduced Dual Inline Memory Module
10. NAS- Network Attached Storage
11. NFS - Network File System
12. NIC - Network Interface Controller (or Card)
13. PCIe - PCI (Peripheral Component Interconnect) Express
14. PERC – (Dell) PowerEdge RAID Controller
15. NVMe – Non-Volatile Memory Express
16. RAID - Redundant Array of Independent Disks
17. SATA - Serial Advanced Technology Attachment
18. SAS - Serial-attached SCSI
19. SCSI - Small Computer System Interface
20. SFP - Small Form Factor Pluggable
21. SSD - Solid State Drive
22. TB - Terabyte
23. VMS - Video Management System B	Reference Standards
1. Institute of Electronic and Electrical Engineers (IEEE) 802.3 standards
2. FCC - Code of Federal Regulations, Title 47, Part 15 C	Definitions
1. iDRAC - Dell technology which allows administrators to deploy, monitor, manage, configure, update, troubleshoot and remediate servers from any location, and without the use of agents, regardless of operating system or hypervisor presence or state.
2. M.2 – Formerly known as NGFF ("Next-Generation Form Factor"), an expansion slot/form factor that can interface with SATA 3.0, PCI Express 3.0, and USB 3.0.
1.04 Submittals
1. Informational Submittals
a. Product Data
1) Manufacturer product data sheets
2) Manufacturer product instructions, and installation and operating manuals
b. Shop Drawings
2. Closeout Submittals
a. Final listing of devices and settings

b. Complete set of supplier’s operating instructions, installation instructions, and troubleshooting guide.
c. Recommended spare parts list. B	Quality Assurance
1. Contractor qualifications: minimum of 2 (two) years system design, engineering supervision, and installation experience in the security or information technology industry.
2. Manufacturer qualifications
a. The Manufacturer shall have a minimum of 5 years of manufacturing, selling and supporting systems of the type described herein and provide evidence of successful installations acceptable to the Owner.
C	Product Delivery, Storage, and Handling
1. Acceptance: Upon delivery to the site, Contractor shall inspect all products and materials for any damage.
1.05 Project Conditions
1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer.
1.06 [bookmark: 1.06_Warranty_and_Support]Warranty and Support
A	This product is covered by a 3-Year, 24/7 Support with Advanced Next-Day Replacement.
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[bookmark: PART__2_PRODUCTS]PART 2	PRODUCTS
2.01 Manufacturer
A BCDVideo
901 Deerfield Pkwy, Buffalo Grove, IL 60089 Phone: +1 847 205-1922
support@bcdvideo.com https://www.bcdvideo.com
B Products
1. 1U 24 port Network Switch	BCD ALE 6360 p24
2.02 Description (General)
A The Switch shall support zero touch configuration.
B Switching shall support LACP 802.3ad.
C Advanced layer-2+ features with basic layer-3.
D Switching shall support IEEE 802.3af, IEEE 802.3at and IEEE802.3bt.
Switch Technical Specifications
E POE+ Network Ports
a. Number:	<24>
b. Type:	10/100/1000 Base-T
F Additional Ports 
1. (1) USB Port, (1) Console Port
2. (2) 1Gb Combo Gigabit RJ45/SFP ports
3. (2) 1Gb/10Gb Fixed SFP/SFP+ uplink
G Power Supply
1. (1) Internal 222W
H Switch Performance
1. Max Switching Capacity: 	128Gb/s 
2. Latency:			Sub 4 μs
I Mean Time Between Failure (MTBF)
1. At 25°C: 			1,447 h
J Environmental
1. Operating temperature: 	0°C to 45°C (32°F to 113°F)
2. Storage Temperature:		-40°C to 85°C (-40°F to 167°F)
3. Operating humidity:		5 to 95% non-condensing


K Mechanical
1. Dimensions:		Width 44.0 cm (17.33 in)
		Depth 22 cm (8.66 in.)
		Height 4.4 cm (1.73 in.)
2. Weight:			3.2 kg (7 lb)
L Electrical
1. Power: 90V to 220V AC
a. Power Supplies:		AC = 1 x 222W
b. POE Power Available:	180W
c. Max Heat Dissipation:	758 BTU/hr.

END OF SECTION


[bookmark: PART__3_EXECUTION]PART 3	EXECUTION

3.01 Installers
A	Contractor personnel shall comply with all applicable state and local licensing requirements. B	Contractor personnel shall comply with all applicable Manufacturer training certifications.
3.02 [bookmark: 3.02_Preparation][bookmark: A_The_network_design_and_configuration_s]Preparation
A [bookmark: B_All_applicable_operating_system_update]The network design and configuration shall be verified for compatibility and performance with the Recording Server.
B All applicable operating system updates available from the Manufacturer shall be installed by the Contractor prior to project completion.

3.03 Installation
A	Contractor shall follow manufacturer published installation and configuration instructions and guidelines.

3.04 Storage
A	Server and system hardware devices and components shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
3.05 Cyber Security
A	AOS Secured Diversified Code Protection
· protects networks from intrinsic vulnerabilities, code exploits, embedded malware, and potential back doors that could compromise mission critical operations.
· defense approach toward network security that continuously defines and implements value-add capabilities to address both current and future threats.

END OF SECTION





Changes since last version of this document:
Note: All changes so far to this document are formatting & layout so don’t affect the specifications in any way.
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