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A&E 2020 Specification
BCDT08-PVS
Professional 8-Bay Tower Video Recording Server



Notes to Specifier:

1. Where several alternative parameters or specifications exist, or where, the specifier has the option of selecting and inserting text, such choices are presented in <bold text>.

2. Explanatory notes and comments are presented in italic text.

3. If there are any changes between the previous version of this document & this updated version (2020), they are listed on the last page of this document.

4. Ref section 3.05 (Cyber Security) Section B. This section has several optional points that will be specific to each site. Please review & include any that are required.














VIDEO RECORDING SERVERS

[bookmark: PART__1_GENERAL]PART 1	GENERAL
1.01 Summary
A	This specification describes an 8-bay tower enterprise class video recording server with capacity up to 128TB SATA.
1.02 Related Requirements
A	23 00 00 Heating, Ventilating, and Air Conditioning (HVAC)
1. 23 70 00	Central HVAC Equipment
2. 23 80 00	Decentralized HVAC Equipment B	27 00 00	Communications
1. 27 05 00	Common Work Results for Communications
2. 27 11 16	Communications Cabinets, Racks, Frames, and Enclosures
3. 27 15 01	Communications Horizontal Cabling Applications
a. 27 15 01.13	Video Surveillance Communications Conductors and Cables
4. 27 21 00	Data Communications Network Equipment
C	28 01 00	Operation and Maintenance of Electronic Safety and Security
1. 28 01 20	Operation and Maintenance of Video Surveillance D	28 05 00	Common Work Results for Electronic Safety and Security
	1. 28 05 07
	Power Sources for Electronic Safety and Security

	2. 28 05 09
	Surge Protection for Electronic Safety and Security

	3. 28 05 11
	Cyber Security Requirements for Electronic Safety and Security

	4. 28 05 17
	Workstations for Electronic Safety and Security

	5. 28 05 19
	Storage Appliances for Electronic Safety and Security

	6. 28 05 31
	Communications Equipment for Electronic Safety and Security

	7. 28 05 45
	Systems Integration and Unified Systems


E 28 06 00	Schedules for Electronic Safety and Security
F 28 08 00	Commissioning of Electronic Safety and Security G	28 20 00	Video Surveillance
1.03 References
A	Abbreviations
1. Gb/s - Gigabit per second
2. GbE - Gigabit Ethernet
3. GB - Gigabyte
4. HDD - Hard Disk Drive
5. iDRAC - Integrated Dell Remote Access Controller
6. LAN - Local Area Network
7. LOM – LAN on Motherboard
8. LRDIMM - Load-Reduced Dual Inline Memory Module
9. NAS- Network Attached Storage
10. NFS - Network File System
11. NIC - Network Interface Controller (or Card)
12. PCIe - PCI (Peripheral Component Interconnect) Express
13. PERC – (Dell) PowerEdge RAID Controller
14. NVMe – Non-Volatile Memory Express
15. RAID - Redundant Array of Independent Disks
16. SATA - Serial Advanced Technology Attachment
17. SAS - Serial-attached SCSI
18. SCSI - Small Computer System Interface
19. SFP - Small Form Factor Pluggable
20. SSD - Solid State Drive
21. TB - Terabyte
22. VMS - Video Management System B	Reference Standards
1. Institute of Electronic and Electrical Engineers (IEEE) 802.3 standards
2. FCC - Code of Federal Regulations, Title 47, Part 15 C	Definitions
3. iDRAC - Dell technology which allows administrators to deploy, monitor, manage, configure, update, troubleshoot and remediate servers from any location, and without the use of agents, regardless of operating system or hypervisor presence or state.
4. Harmonize iDRAC Plug-In – Software provided by BCD that displays the alarms & alerts within the VMS & displayed in the client. This simplifies the management of a system, reduces risk in missing faults and provides predictive failures.
5. Harmonize Bridge - Powered by Tiger Technology, to provide on-premise storage, off-site Cloud storage and Disaster Recovery.
6. M.2 – Formerly known as NGFF ("Next-Generation Form Factor"), an expansion slot/form factor that can interface with SATA 3.0, PCI Express 3.0, and USB 3.0.
7. Cyber Security - Computer security or information technology security is the protection of computer systems and networks from information disclosure, theft of or damage to their hardware, software, or electronic data, as well as from the disruption or misdirection of the services they provide.
1.04 Submittals
1. Informational Submittals
a. Product Data
1) Manufacturer product data sheets
2) Manufacturer product instructions, and installation and operating manuals
b. Shop Drawings
2. Closeout Submittals
a. Final listing of devices and settings
b. Complete set of supplier’s operating instructions, installation instructions, and troubleshooting guide.
c. Recommended spare parts list. B	Quality Assurance
1. Contractor qualifications: minimum of 2 (two) years system design, engineering supervision, and installation experience in the security or information technology industry.
2. Manufacturer qualifications
a. The Manufacturer shall have a minimum of 5 years of manufacturing, selling and supporting systems of the type described herein and provide evidence of successful installations acceptable to the Owner.
C	Product Delivery, Storage, and Handling
1. Acceptance: Upon delivery to the site, Contractor shall inspect all products and materials for any damage.
1.05 Project Conditions
1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer.
1.06 [bookmark: 1.06_Warranty_and_Support]Warranty and Support
A	Manufacturer shall provide a five-year, on-site, next business day warranty, with a “Keep Your Hard Drive” feature.
Keep Your Hard Drive is defined as: In the event of a drive failure, a replacement drive shall be provided, and the faulty drive shall remain on premise.
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[bookmark: PART__2_PRODUCTS]PART 2	PRODUCTS
2.01 Manufacturer
A BCDVideo
901 Deerfield Pkwy, Buffalo Grove, IL 60089 Phone: +1 847 205-1922
support@bcdvideo.com https://www.bcdvideo.com
B Products
1. 8 Bay Tower Video Recording Servers	BCDT08-PVS
2.02 Description
A The Video Recording Server (“Recording Server”) shall be an enterprise class 8-bay tower server providing storage scalability up to 128TB of RAW storage (SATA).
B The Manufacturer shall certify that the Recording Server has been designed and built for the purpose of recording surveillance video.
C The Platform shall provide the capability for remote management, disaster recovery, and critical resource management.
D The Platform shall have dual dedicated operating system drives to facilitate accelerated boot and application load times.
E The Platform shall have redundant, hot-swappable, storage drives, cooling fans and power supplies.
F Video Storage
1. Hard Drive Bays
a. Number:	8
b. Type:	Enterprise SATA Drives
2. SAS Drives:
a. Size:	3.5”
b. Capacity:	N/A
c. Speed:	7200 rpm
3. SATA Drives:
a. Size:	3.5”
b. Capacity	4TB, 8TB, 10TB, 12TB, 14TB or 16TB per drive
c. Speed:	7200 rpm
4. High-Performance 10K SAS Drives
a. Size:	2.5”
b. Capacity:	N/A
c. Speed:	10000 rpm
5. High-Performance 15K SAS Drives
a. Size:	2.5”
b. Capacity:	N/A
c. Speed:	15000 rpm
G Processor
1. Number:	<1> Intel® Xeon® E-2226G Processor
2. Properties:	6 Cores, 6 Threads, 4.70 GHz 
H Operating System
1. Software:	Windows Server 2019
2. Drives:	2 x 240GB 2.5” M.2 NVMe SSD dedicated, RAID 1 configured
I Video Management System – The Recording Server shall have the VMS pre-installed and configured at the assembly location.
J Harmonize software suite
1. Harmonize iDRAC Plug-In – Software provided by BCD that displays the alarms & alerts within the VMS & displayed in the client. This simplifies the management of a system, reduces risk in missing faults and provides predictive failures.
2. Harmonize Bridge – Powered by Tiger Technology, to provide on-premise storage, off-site Cloud storage and Disaster Recovery.
K Memory
1. 16GB as standard. Up to <64 GB> in 8 GB increments, <64 GB> in 16GB increments.
L Network Controller
1. Ports: (2) 1GbE RJ45
2. Remote Management: via dedicated iDRAC port (Front: Micro-AB USB, Rear: RJ45)
M Additional Ports
1. Video output:	VGA (1)
2. USB:	Rear (2) USB 3.0, (4) USB 2.0; Front (1) USB 3.0, (1) USB 2.0
N Redundancy and Resilience
1. RAID
a. Levels supported:	RAID 0, 1, 5, 6, 10
b. Controller:	PERC H730P (2GB NV Cache)
O Electrical
1. Power: 100–240 V AC, auto-ranging
a. Power Supplies:	2 x <495> W
b. Heat Dissipation:	<1908> BTU/hr
P Mechanical
1. Dimensions (w x d x h): 	8.58" (218mm) x 22.18" (589.1mm) x 18.56" (471.3mm)
2. Weight:	57.32 pounds (26 kg)
3. Form factor:	Standalone tower with 4U rack-mount options
4. Rack support:	sliding rack rail with cable management arm
Q Environmental
1. Operating temperature: 50°F - 95° F (10°C - 35°C)
2. Operating humidity:	10 – 80% non-condensing


END OF SECTION
[bookmark: PART__3_EXECUTION]
PART 3	EXECUTION

3.01 Installers
A	Contractor personnel shall comply with all applicable state and local licensing requirements. B	Contractor personnel shall comply with all applicable Manufacturer training certifications.
3.02 [bookmark: 3.02_Preparation][bookmark: A_The_network_design_and_configuration_s]Preparation
A [bookmark: B_All_applicable_operating_system_update]The network design and configuration shall be verified for compatibility and performance with the Recording Server.
B All applicable operating system updates available from the Manufacturer shall be installed by the Contractor prior to project completion.

3.03 Installation
A	Contractor shall follow manufacturer published installation and configuration instructions and guidelines.

3.04 Storage
A	Server and system hardware devices and components shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
3.05 Cyber Security
A Build Cycle…
· CVE updated and patched system images
· Ongoing system image updates and security evaluations
· Digitally signed UEFI driver’s firmware updates
B	Build Cycle (Optional, please check if they are relevant to your site’s specifications)…
· Hardware root of trust enabled with secure boot options
· Optional system secure boot with TPM enabled features
· Operating system secure boot policy enabled options
· Optional hard drive encryption and enterprise key management
· TAA/NDAA compliant hardware is available
· Optional limited hardware ports of entry
C	Supply Chain Security…
· Direct and in-channel equipment sourcing from ODM and OCM partners
· CCTV monitored warehouse, staging and build facilities to ensure no tampering
· Controlled access to facilities
· Screening and inspection of cargo at entry



END OF SECTION
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